For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement.
2. Disconnect the evaporative emission (EVAP) canister purge line quick connect fitting (1) at the chassis line. Refer to Plastic Collar Quick Connect Fitting Service.
3. Remove the EVAP canister purge line.

### Installation Procedure

1. Install the EVAP canister purge line.
2. Connect the EVAP canister purge line quick connect fitting (1) to the chassis. Refer to Plastic Collar Quick Connect Fitting Service.
3. Install the fuel tank. Refer to Fuel Tank Replacement.