For 1990-2009 cars

### System Description

The horn system consists of the following components:

• | Horn relay

• | Horn switch

• | Horn

• | Body control module (BCM)

### System Operation

• | The vehicle horn is activated whenever the horn switch is depressed.

• | The BCM commands the horn ON under any of the following conditions:

- | When the panic button is depressed on the remote control door lock transmitter. For further information refer to Keyless Entry System Description and Operation.

- | When the content theft deterrent system detects a vehicle intrusion. For further information refer to Content Theft Deterrent (CTD) Description and Operation.

- | When the keyless entry system is used to lock the vehicle, a horn chirp may sound to notify the driver that the vehicle has been locked. The notification feature may be enabled or disabled through personalization. For further information refer to Keyless Entry System Description and Operation.

### Circuit Operation

Battery positive voltage is applied at all times to the horn relay coil and the horn relay switch. Pressing the horn switch applies ground to the horn switch signal circuit. The BCM also may apply ground to the horn relay control circuit as described above. When the horn relay control circuit is grounded, the horn relay is energized and battery positive voltage is applied to the horn through the horn control circuit. The horn will sound as long as ground is applied to the horn relay control circuit.