For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
3. Remove the drive belt. Refer to Drive Belt Replacement.

1 | Engine Harness Generator Connector
2 | Engine Harness Ground Terminal Boot
3 | Engine Harness Ground Terminal Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
4 | Engine Harness Ground Terminal
5 | Generator Bolt (Qty: 3) Tighten 22 N·m (16 lb ft)
6 | Generator