For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.

1 | Inflatable Restraint Instrument Panel (I/P) Module Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Open the I/P storage compartment to access bolts.

Tighten
10 N·m (89 lb in)

2 | Inflatable Restraint Instrument Panel (I/P) Module Assembly Warning: Refer to SIR Warning in the Preface section. Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section.

#### Procedure

1. Disconnect the electrical connector.
2. After replacing the module, deploy the old module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping.