For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the charge air cooler inlet pipe if equipped. Refer to Charge Air Cooler Inlet Pipe Replacement.
2. Remove the charge air cooler outlet pipe if equipped. Refer to Charge Air Cooler Outlet Pipe Replacement.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Radiator Air Deflector Bolt - Front (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Radiator Air Deflector Assembly - Front
3 | Air Inlet Shroud Retainer (Qty: 2)
4 | Air Inlet Shroud