For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Fully lower the door window before removing the trim panel.

1 | Mirror Outside Rearview Nut (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tip Disconnect the mirror electrical connector. Tighten
10 N·m (89 lb in)

2 | Outside Rearview Mirror Assembly