For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptors

DTC B1325 03 : Device Power 1 Circuit Voltage Below Threshold
DTC B1325 07: Device Power 1 Circuit Voltage Above Threshold

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
B+ | B1325 03 | B1325 03 | -- | --
Ground | -- | B1325 03 | -- | --

### Circuit/System Description

The following control modules monitor the system voltage through the battery positive (B+) voltage circuits:

• | Body Control Module (BCM)

• | Inflatable restraint sensing and diagnostic module (SDM)

• | Instrument panel cluster (IPC)

• | Radio

### Conditions for Running the DTC

• | The voltages supplied to the control modules are in the range of 7-26 V.

• | The ignition is ON.

### Conditions for Setting the DTC

#### B1325 03

The control module detects a system voltage less than 9 V 5 seconds.

#### B1325 07

The control module detects a system voltage greater than 18 V for 5 seconds.

### Conditions for Clearing the DTC

The DTC passes when the malfunction is no longer present.

### Diagnostic Aids

• | A high or low voltage value in multiple modules indicates a concern in the charging system.

• | Overcharging with a battery charger or jump starting can cause this DTC to set.

### Reference Information

#### Schematic Reference

• | Body Control System Schematics

• | Radio/Navigation System Schematics

• | Instrument Cluster Schematics

• | SIR Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Charging System Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Testing

1. Engine running, accessories OFF, measure and record the battery voltage at the battery terminals. The voltage should be between 12.6 and 15.0 V.

⇒ | If the battery voltage is not within the specified range, refer to Charging System Test

2. Ignition OFF, disconnect the harness connectors of the appropriate control module.
3. Ignition OFF and scan tool disconnected, open and close the driver door, and wait 1 minute.
4. Test for less than 5.0 Ω between the ground circuit and ground.

• | Terminal 61 X1 Terminal E12 X4 (BCM)

• | Terminal 31 (SDM)

• | Terminal 15 (IPC)

• | Terminal 8 X2 (Radio)

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

5. Ignition ON, verify a test lamp illuminates between the B+ circuit and ground.

• | Terminals D1-D12 X3 (BCM)

• | Terminals 1-33 (SDM)

• | Terminals 11-13 (IPC)

• | Terminal 1 X2 (Radio)

⇒ | If the test lamp does not illuminate , test the B+ circuit for a short to ground or an open/high resistance.

6. If all circuits test normal, replace the appropriate control module.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Control Module References for the appropriate control module replacement, setup, and programming.