For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) carrier. Refer to Instrument Panel Carrier Replacement.
2. Pull the tie bar far enough back for the air distribution duct to clear the opening.
3. Remove the I/P tie bar. Refer to Instrument Panel Tie Bar Replacement.

1 | Distributor Air Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Distributor Air Nut (Qty: 3) Tighten 2.5 N·m (22 lb in)
3 | Distributor Air Bolt Tighten 2.5 N·m (22 lb in)
4 | Air Distributor