For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Reach in between the bumper and front hood opening and rotate the park turn bulb socket counterclockwise a quarter turn, and remove.

1 | Park and Turn Signal Lamp Bulb Socket Procedure Rotate the bulb socket counterclockwise from the lamp housing in order to remove.
2 | Park and Turn Signal Lamp Bulb Tip Pull the bulb straight from the socket in order to remove the bulb from the lamp socket.