For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Nut | 10 N·m | 89 lb in
Air Cleaner Front Bolt/Nut | 10 N·m | 89 lb in
Air Cleaner Outlet Duct Clamp | 4 N·m | 35 lb in
Air Inlet Screen Support Nut | 10 N·m | 89 lb in
Brake Pipe | 20 N·m | 15 lb ft
Camshaft Position Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Charge Air Cooler Bolt | 9 N·m | 80 lb in
Charge Air Cooler Hose Clamp | 6 N·m | 53 lb in
Charge Air Cooler Pipe Clamp | 5 N·m | 44 lb in
Charge Air Cooler Pipe Bolt | 7 N·m | 62 lb in
Charge Air Cooler Rear Bracket Nut | 9 N·m | 80 lb in
Charge Air Bypass Solenoid Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Purge Solenoid Bolt | 10 N·m | 89 lb in
Fuel Feed Pipe Bolt | 10 N·m | 89 lb in
Fuel Feed Pipe Fitting | 30 N·m | 22 lb ft
Fuel Fill Hose Clamp | 4.5 N·m | 40 lb in
Fuel Fill Pipe Ground Strap Bolt | 9 N·m | 80 lb in
Fuel Fill Pipe to Housing Bolt | 1.5 N·m | 13 lb in
Fuel Injector Fuel Rail Fuel Pressure Sensor | 33 N·m | 25 lb ft
Fuel Pump Module Access Cover Bolt | 10 N·m | 89 lb in
Fuel Rail Bolt | 22 N·m | 16 lb ft
Fuel Tank Strap/Support Bolt | 25 N·m | 18 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
High Pressure Fuel Feed Pipe Fitting | 32 N·m | 24 lb ft
High Pressure Fuel Pump Cover Bolt | 10 N·m | 89 lb in
High Pressure Fuel Pump Bolt | 15 N·m | 11 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Air Pressure and Temperature Sensor Bolt | 9 N·m | 80 lb in
Knock Sensor | 25 N·m | 18 lb ft
Manifold Absolute Pressure (MAP) Sensor Bolt | 10 N·m | 89 lb in
Mass Air Flow (MAF) Sensor Screw | 0.6 N·m | 5 lb in
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in