For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the fuse labeled HVAC CTRL (BATT).
2. Remove the instrument panel (I/P) carrier. Refer to Instrument Panel Carrier Replacement.

1 | Recirculation Housing Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Recirculation Housing
3 | Recirculation Actuator Screw (Qty: 3) Tighten 1.5 N·m (13 lb in)
4 | Recirculation Actuator

#### Procedure

• | Disconnect the actuator electrical connector.

• | Recalibrate the actuator. Refer to Actuator Recalibration