For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Secure the steering wheel utilizing a strap to prevent rotation. Locking of the steering column will prevent damage and a possible malfunction of the SIR system. The steering wheel must be secured in position before disconnecting the following components:

• | The steering column

• | The intermediate shaft

• | The steering gear

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.

#### Preliminary Procedures

1. Remove the left front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
2. Remove the driver knee bolster bracket. Refer to Driver Knee Bolster Bracket Replacement .

1 | Intermediate Steering Shaft Bolt Notice: Refer to Fastener Notice in the Preface section. Tip Discard the bolt. Tighten
58 N·m (43 lb ft)

2 | Intermediate Steering Shaft Lower Bolt Tip Discard the bolt. Tighten 58 N·m (43 lb ft)
3 | Intermediate Steering Shaft Seal Tip Make sure the seal is seated properly when installing.
4 | Intermediate Steering Shaft