For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the driver knee bolster bracket. Refer to Driver Knee Bolster Bracket Replacement .
2. Lower the steering column as necessary. Refer to Steering Column Replacement .

1 | Steering Column Upper Trim Cover
2 | Steering Column Upper Trim Cover Retainer (Qty: 2)
3 | Steering Column Lower Trim Cover Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
4 | Steering Column Lower Trim Cover
5 | Steering Column Lower Trim Cover Bolt Tighten 2.5 N·m (22 lb in)
6 | Steering Column Lower Trim Cover
7 | Steering Column Lower Trim Cover Plug