For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.
3. Remove the energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement.
4. Remove the front bumper impact bar bracket. Refer to Front Bumper Impact Bar Bracket Replacement.

1 | Front Impact Bar Bolt (Qty: 8) Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Front Impact Bar Bolt (Qty: 4) Tighten 9 N·m (80 lb in)
3 | Front Impact Bar