For 1990-2009 cars

### Circuit/System Testing

1. Remove the flywheel inspection cover.
2. Inspect the flywheel for the following:

• | Loose flywheel bolts

• | Chipped gear teeth

• | Missing gear teeth

• | Bent flywheel

⇒ | If not within specifications, secure the flywheel bolts or replace the flywheel.

⇒ | If all inspections were within specification, replace the starter motor.

### Repair Instructions

• | Fastener Tightening Specifications for the 2.0L engine.

• | Engine Flywheel Replacement for the 2.0L engine.

• | Starter Motor Replacement