For 1990-2009 cars

## Cooling Fan Always On 2.0

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Circuit/System Description

The engine cooling fan is a variable speed fan. The engine control module (ECM) controls the fan speed by sending a pulse width modulated (PWM) signal to the cooling fan control module. The cooling fan control module varies the voltage drop across the engine cooling fan motor in relation to the pulse width modulated signal. The cooling fan speed can be adjusted from 10 percent to 90 percent duty cycle. 90-94 percent is considered high speed fan.

The ECM monitors the voltage on the cooling fan speed control circuit driver output. Voltage is near B+ when the driver is OFF, and near ground when the driver is ON. If the difference between the actual and expected voltage exceeds a calibrated value, a DTC will set.

### Reference Information

#### Schematic Reference

Engine Cooling Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Cooling Fan Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. If DTCs P0480, P0691, or P0692 are set, perform that diagnostic first.
2. Ignition ON, verify with a scan tool that the ECM is not commanding fan activation.
3. Ignition ON, observe that the fan is not activated.

⇒ | If the fan is activated, replace the cooling fan assembly.

### Repair Instructions

Perform the Cooling Fan and Shroud Replacement after completing the diagnostic procedure.

### Repair Verification

1. Ignition ON, verify with a scan tool that the ECM is not commanding fan activation.
2. Ignition ON, observe that the fan is not activated.