For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air inlet grill panel. Refer to Air Inlet Grille Panel Replacement .

1 | Radiator Surge Tank Hose Assembly - Outlet

#### Procedure

Using J 38185 position radiator surge tank outlet hose clamps aside and remove hose from the fittings.

#### Special Tools

J 38185 Hose Clamp Pliers