For 1990-2009 cars

### Removal Procedure

1. Remove the turbocharger. Refer to Turbocharger Replacement.
2. Remove the exhaust manifold heat shield bolts.
3. Remove the heat shield.
4. Remove and discard the exhaust manifold nuts.
5. Remove the exhaust manifold.
6. Remove and discard the exhaust manifold gasket.

### Installation Procedure

1. Install a NEW exhaust manifold gasket onto the studs.
2. Install the exhaust manifold.
3. Install the NEW exhaust manifold nuts.

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the exhaust manifold nuts in the sequence shown to 14 N·m (10 lb ft).
5. Install the heat shield.
6. Install the exhaust manifold heat shield bolts and tighten to 25 N·m (18 lb ft).
7. Install the turbocharger. Refer to Turbocharger Replacement.