For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
2. Remove the rear bumper fascia bracket. Refer to Rear Bumper Fascia Bracket Replacement.

1 | Rear Bumper Fascia Center Bracket Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (17 lb in)
2 | Rear Bumper Fascia Center Bracket