For 1990-2009 cars

### Removal Procedure

1. Disconnect the engine wiring harness electrical connector (4) from the exhaust camshaft position (CMP) sensor.
2. Remove the CMP sensor bolt. (Intake CMP shown, exhaust CMP similar)
3. Remove the CMP sensor.

### Installation Procedure

Note: Inspect the CMP sensor for damage. Replace as necessary.

1. Lubricate the CMP sensor O-ring seal with clean engine oil.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CMP sensor. (Intake CMP shown, exhaust CMP similar)
3. Install the CMP sensor bolt and tighten to 10 N·m (89 lb in).
4. Connect the engine wiring harness electrical connector (4) to the exhaust CMP sensor.