For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Position window approximately half way down.
2. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
3. Remove the water deflector. Refer to Door Water Deflector Replacement.

1 | Front Side Door Window Regulator to Window Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Door Window Tip Adjust the door window. Refer to Door Window Adjustment.