For 1990-2009 cars

## Front Wheelhouse Liner Replacement Base

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheel. Refer to Tire and Wheel Removal and Installation.

1 | Front Wheelhouse Liner Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Wheelhouse Liner Screws (Qty: 6)
3 | Front Wheelhouse Liner Retainers (Qty: 3)
4 | Front Wheelhouse Liner