For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
4. Remove the generator. Refer to Generator Replacement.

1 | A/C Compressor and Condenser Hose Assembly Nut Caution: Refer to Fastener Caution in the Preface section. Tip A/C compressor hose to A/C evaporator hose Tighten
9 N·m (80 lb in)

2 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor and Condenser Hose Assembly Nut Tip A/C compressor hose to A/C condenser Tighten 9 N·m (80 lb in)
4 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement.

5 | A/C Compressor and Condenser Hose Assembly Bolt Tighten 22 N·m (16 lb ft)
6 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement.

7 | A/C Compressor and Condenser Hose Assembly