For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement .
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
4. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .

1 | A/C Condenser Tube Assembly Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

3 | Push Pin Retainer
4 | A/C Condenser Tube Assembly Nut Tighten 9 N·m (80 lb in)
5 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

6 | A/C Condenser Tube Assembly