For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the fuse labeled HVAC CTRL (BATT).
2. Remove the I/P Insulator Panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | Air Temperature Actuator Screw - Left (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Air Temperature Actuator - Left

#### Procedure

• | Disconnect the actuator electrical connector.

• | Recalibrate the actuator. Refer to Actuator Recalibration