For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement.

1 | Radio Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | AM/FM Stereo Radio Assembly

#### Procedure

Program the radio after replacement. Refer to Control Module References.