For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the brake cooling duct retainer.

1 | Front Fascia Retainer (Qty: 12)
2 | Front Fascia Screw (Qty: 22) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Fascia Bracket Screw (Qty: 4) Tighten 2 N·m (18 lb in)
4 | Front Fascia Center Bracket Retainer
5 | Front Fascia Tip Disconnect the lamp connectors.