For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Partially remove the side rear weatherstrip for access to the retainer screws. Refer to Folding Top Side Rear Weatherstrip Replacement .

1 | Folding Top Side Rear Weatherstrip Retainer Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Folding Top Side Rear Weatherstrip Retainer Tip

• | If necessary, adjust the weatherstrip retainer. Refer to Folding Top Side Front Weatherstrip Retainer and Side Rear Weatherstrip Retainer Adjustment .

• | Inspect the fit of the seal to door glass.

• | Cycle the top and inspect the joint between side front/rear rail weatherstrips.