For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.

1 | Front Fascia Reinforcement Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Fascia Reinforcement Bolt (Qty: 2)
3 | Front Fascia Reinforcement Tip Remove the screws from the end of the fascia and then remove the reinforcement.
4 | Front Fascia Bracket Bolt
5 | Front Fascia Bracket
6 | Front Fascia Bracket Bolt
7 | Front Fascia Bracket