For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console. Refer to Front Floor Console Replacement.
2. With the park brake lever fully released, completely back off the cable adjustment nut.

The park brake cable adjusting nut is a nylon lock type. Use ONLY HAND TOOLS whenever tightening or loosening the adjusting nut.

3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Park Brake Cable

#### Procedure

1. Carefully position the driveline tunnel insulator downward just enough to access the cable equalizer.
2. Rotate the front cable end to release the cable from the equalizer.

2 | Park Brake Lever Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
3 | Park Brake Lever Assembly

#### Procedure

1. Disconnect the electrical connector from the park brake warning lamp switch.
2. Adjust the tension of the park brake cables. Refer to Park Brake Adjustment.