For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the charge air cooler. Refer to Charge Air Cooler Replacement.
3. Remove the lower radiator air baffle. Refer to Radiator Air Lower Baffle and Deflector Replacement.
4. Remove the upper radiator air baffle. Refer to Radiator Air Upper Baffle and Deflector Replacement.

1 | Receiver Dehydrator Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Receiver Dehydrator Screw Tighten 1.5 N·m (13 lb in)
3 | Receiver Dehydrator O-Ring

#### Procedure

Remove and discard the O-rings.

4 | Receiver Dehydrator Assembly