For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.
4. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | A/C Condenser Tube Assembly Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

3 | Push Pin Retainer
4 | A/C Condenser Tube Assembly Nut Tighten 9 N·m (80 lb in)
5 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

6 | A/C Condenser Tube Assembly