For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the door trim panel. Refer to Door Trim Panel Replacement.
2. Remove the door mirror face. Refer to Outside Rearview Mirror Glass Replacement.

1 | Front Door Mirror Motor Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Door Mirror Motor Tip Disconnect the electrical connector from the mirror motor.