For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) upper trim panel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement.

1 | Heater and Air Conditioning Control Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
2 | Heater and Air Conditioning Control Assembly

#### Procedure

Disconnect the control module electrical connectors.