For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.

1 | Front Park and Turn Signal and Fog Lamp Assembly Screws (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Park and Turn Signal and Fog Lamp Assembly Tip Disconnect and remove the electrical jumper harness, bulbs and remove the lamp assembly from inside the front bumper fascia.