For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Door Water Deflector Replacement.
3. Move the window to the full up position.

1 | Front Side Door Check Link Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Check Link Nut (Qty: 2) Tighten 10 N·m (89 lb in)
3 | Front Side Door Check Link Assembly Tip Remove the check link from the inside of the door.