For 1990-2009 cars

#### Special Tools

• | J 43653 Flywheel Holding Tool

• | J 45059 Angle Meter

### Removal Procedure

1. Remove the engine drive belt. Refer to Drive Belt Replacement.
2. Remove the starter motor. Refer to Starter Motor Replacement.
3. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
4. Install the J 43653 (1) to the engine block, in order to hold the flywheel.
5. Remove the crankshaft balancer bolt. Discard the bolt.
6. Remove the balancer using a universal removal tool.

### Installation Procedure

Caution: Ensure both components are aligned correctly or serious engine damage will occur.

1. Install the crankshaft balancer onto the crankshaft indexing keyway. Use care to properly align the keyway and the flats on the balancer with the oil pump drive.
2. Install the crankshaft balancer using a universal balancer installer.

Caution: Refer to Fastener Caution in the Preface section.

Note: Always install a NEW crankshaft balancer bolt and washer.

3. Install a NEW crankshaft balancer bolt. Prevent the crankshaft from rotating when tightening the bolt.

Tighten the bolt to 100 N·m (74 lb ft) plus an additional 125 degrees using the J 45059 .

4. Remove the J 43653 (1) from the engine block.
5. Lower the vehicle.
6. Install the starter motor. Refer to Starter Motor Replacement.
7. Install the engine drive belt. Refer to Drive Belt Replacement.