For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement.

1 | Air Outlet Duct Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the actuator electrical connectors from the recirculation case.

Tighten
1.5 N·m (13 lb in)

2 | Air Outlet Duct
3 | Heater Core Cover Screw (Qty: 2) Tighten 1.5 N·m (13 lb in)
4 | Heater Core Cover
5 | Heater Core Pass Through Seal
6 | Air Distribution Case Screw (Qty: 5) Tighten 1.5 N·m (13 lb in)
7 | Air Distribution Case
8 | Heater Core Tube Clamp Screw (Qty: 2)
9 | Heater Core Tube Clamp
10 | Heater Core