For 1990-2009 cars

1. Loosen the rear suspension adjustment link lock nut (1).
2. Rotate the inner tie rod (2) to the required toe specification setting. Refer to Wheel Alignment Specifications.

Caution: Refer to Fastener Caution in the Preface section.

3. Tighten the rear suspension adjustment link lock nut to 60 N·m (44 lb ft).
4. Check the toe setting after tightening.
5. Adjust the toe setting if necessary.