For 1990-2009 cars

Table 1: | Remote Control Door Lock Receiver Scan Tool Data Parameters
Table 2: | Remote Control Lock Receiver Scan Tool Output Controls

#### Remote Control Door Lock Receiver Scan Tool Data Parameters

Parameter | Expected Value | Definition
--- | --- | ---
Operating Conditions: Ignition ON
Fob 1 Battery | OK | The scan tool displays OK or Low. This is the state of the Fob 1 battery.
Fob 1 Function | None | The scan tool displays None, Lock, Dr Door Unlock, All Door Unlock, R Closure Rel., Lt Sliding Ctrl., Rt Sliding Ctrl., Panic, Fuel Door, Power Window, Power Top, Engine Start, Engine Stop, Fob Program, Locate, R Closure Close, R Closure Open, R Closure Stop, Double Lock, R Closure Start or Lt Sliding Stop. This is the state of the Fob 1 command as monitored by the RCDLR.
Fob 1 Programmed | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 1 is programmed into the RCDLR.
Fob 2 Battery | OK | The scan tool displays OK or Low. This is the state of the Fob 2 battery.
Fob 2 Function | None | The scan tool displays None, Lock, Dr Door Unlock, All Door Unlock, R Closure Rel., Lt Sliding Ctrl., Rt Sliding Ctrl., Panic, Fuel Door, Power Window, Power Top, Engine Start, Engine Stop, Fob Program, Locate, R Closure Close, R Closure Open, R Closure Stop, Double Lock, R Closure Start or Lt Sliding Stop. This is the state of the Fob 2 command as monitored by the RCDLR.
Fob 2 Programmed | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 2 is programmed into the RCDLR.
Fob 3 Battery | OK | The scan tool displays OK or Low. This is the state of the Fob 3 battery.
Fob 3 Function | None | The scan tool displays None, Lock, Dr Door Unlock, All Door Unlock, R Closure Rel., Lt Sliding Ctrl., Rt Sliding Ctrl., Panic, Fuel Door, Power Window, Power Top, Engine Start, Engine Stop, Fob Program, Locate, R Closure Close, R Closure Open, R Closure Stop, Double Lock, R Closure Start or Lt Sliding Stop. This is the state of the Fob 3 command as monitored by the RCDLR.
Fob 3 Programmed | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 3 is programmed into the RCDLR.
Fob 4 Battery | OK | The scan tool displays OK or Low. This is the state of the Fob 4 battery.
Fob 4 Function | None | The scan tool displays None, Lock, Dr Door Unlock, All Door Unlock, R Closure Rel., Lt Sliding Ctrl., Rt Sliding Ctrl., Panic, Fuel Door, Power Window, Power Top, Engine Start, Engine Stop, Fob Program, Locate, R Closure Close, R Closure Open, R Closure Stop, Double Lock, R Closure Start or Lt Sliding Stop. This is the state of the Fob 4 command as monitored by the RCDLR.
Fob 4 Programmed | Yes | The scan tool displays Yes or No. Yes is displayed if the Fob 4 is programmed into the RCDLR.
Front Placard | Varies | This displays Counts.
Last Fob Used | Varies | The scan tool displays None, Fob 1, Fob 2, Fob 3, Fob 4 or Fob 5. This was the last Fob used, as monitored by the RCDLR.
Learn in Progress | Yes | The scan tool displays Yes or No. This is the status of the key fob.
LF Pressure Sensor Mode | Varies | The scan tool displays Learn, Re-measure, Rolling, Entering Off or Exiting Off. This is the state of the left front pressure sensor.
LF Pressure Status | Normal | The scan tool displays Unknown, Normal, Low, Flat or High. This is the state of the left front tire pressure.
LF Tire Press. Sensor Status | Normal | The scan tool displays Normal or Failed. This is the state of the left front tire pressure sensor.
LF Tire Pressure | Varies | This displays kPa (psi). This is the amount of pressure in the left front tire.
LF Tire Pressure Sensor Battery Status | OK | The scan tool displays OK or Low. This is the state of the battery in the left front tire pressure sensor.
LR Pressure Sensor Mode | Varies | The scan tool displays Learn, Re-measure, Rolling, Entering Off or Exiting Off. This is the state of the left rear pressure sensor.
LR Pressure Status | Normal | The scan tool displays Unknown, Normal, Low, Flat or High. This is the state of the left rear tire pressure.
LR Tire Press. Sensor Status | Normal | The scan tool displays Normal or Failed. This is the state of the left rear tire pressure sensor.
LR Tire Pressure | Varies | This displays kPa (psi). This is the amount of pressure in the left rear tire.
LR Tire Pressure Sensor Battery Status | OK | The scan tool displays OK or Low. This is the state of the battery in the left rear tire pressure sensor.
Rear Placard | Varies | This displays Counts.
RF Pressure Sensor Mode | Varies | The scan tool displays Learn, Re-measure, Rolling, Entering Off or Exiting Off. This is the state of the right front pressure sensor.
RF Pressure Status | Normal | The scan tool displays Unknown, Normal, Low, Flat or High. This is the state of the right front tire pressure.
RF Tire Press. Sensor Status | Normal | The scan tool displays Normal or Failed. This is the state of the right front tire pressure sensor.
RF Tire Pressure | Varies | This displays kPa (psi). This is the amount of pressure in the right front tire.
RF Tire Pressure Sensor Battery Status | OK | The scan tool displays OK or Low. This is the state of the battery in the right front tire pressure sensor.
RR Pressure Sensor Mode | Varies | The scan tool displays Learn, Re-measure, Rolling, Entering Off or Exiting Off. This is the state of the right rear pressure sensor.
RR Pressure Status | Normal | The scan tool displays Unknown, Normal, Low, Flat or High. This is the state of the right rear tire pressure.
RR Tire Press. Sensor Status | Normal | The scan tool displays Normal or Failed. This is the state of the right rear tire pressure sensor.
RR Tire Pressure | Varies | This displays kPa (psi). This is the amount of pressure in the right rear tire.
RR Tire Pressure Sensor Battery Status | OK | The scan tool displays OK or Low. This is the state of the battery in the right rear tire pressure sensor.
Selected Front Tire Type | Varies | The scan tool displays N/A, P-Metric (S), P-Metric (X), Load Range C, Load Range D or Load Range E. This is the type of front tires used on the vehicle.
Selected Rear Tire Type | Varies | The scan tool displays N/A, P-Metric (S), P-Metric (X), Load Range C, Load Range D or Load Range E. This is the type of rear tires used on the vehicle.
TPM Indicator/Message | Off | The scan tool displays On or Off. This is the state of the TPM indicator.
TPM System Enabled | Yes | The scan tool displays Yes or No. Yes is displayed if the TPM system is enabled.

#### Remote Control Lock Receiver Scan Tool Output Controls

Scan Tool Output Control | Description
--- | ---
Copy and Paste TPM Information | This procedure copies existing setup information from the module.
Invalidate All Fobs | This program will erase all key fobs from memory and then begin reprogramming.
Next Available Slot | This program will add key fobs being programmed to the first open slot available in the module.
Program Key Fob 1 |

1. Place module in program mode.
2. Repeatedly press and hold the Lock/Unlock buttons on the key fob.

Program Key Fob 2 |

1. Place module in program mode.
2. Repeatedly press and hold the Lock/Unlock buttons on the key fob.

Program Key Fob 3 |

1. Place module in program mode.
2. Repeatedly press and hold the Lock/Unlock buttons on the key fob.

Program Key Fob 4 |

1. Place module in program mode.
2. Repeatedly press and hold the Lock/Unlock buttons on the key fob.

Tire/Type/Pressure Selection |

1. Select load range from list.
2. Select recommended front tire pressure.
3. Select recommended rear tire pressure.