For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: The ball stud must not rotate during disassembly or reassembly. Hand tools must be used to keep the ball stud from rotating. If air tools are used and the stud is allowed to rotate, damage to the ball stud and/or stud mounting hole may occur.

#### Preliminary Procedure

Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Stabilizer Shaft Link Mounting Nuts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 72 N·m (53 lb ft) Tip
Support the lower control arm in order to remove load pressure from the stabilizer link.

2 | Stabilizer Shaft Link