For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the seat belt from the seat. Refer to Seat Belt Retractor Pretensioner Replacement - Front .

1 | Seat Adjuster Nut (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tip Adjust the seat forward or rearward to access the nuts. Tighten
45 N·m (33 lb ft)

2 | Seat Assembly

#### Procedure

Disconnect the electrical connectors.