For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement.

1 | Power Steering Cooler Hose Clamp

#### Procedure

Remove as much power steering fluid from the remote power steering fluid reservoir as possible.

2 | Power Steering Cooler Hose
3 | Power Steering Fluid Reservoir Outlet Hose Clamp
4 | Power Steering Fluid Reservoir Outlet Hose
5 | Remote Power Steering Fluid Reservoir Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
6 | Remote Power Steering Fluid Reservoir

#### Procedure

Fill and bleed the power steering system. Refer to Power Steering System Bleeding