For 1990-2009 cars

## Headlamp Bulb Replacement Hi Beam

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open and support the hood in order to access the headlamp bulb accessory covers and headlamp bulbs.

1 | Headlamp Bulb Accessory Cover Procedure Rotate counterclockwise and remove.
2 | Headlamp Bulb Assembly (Hi) Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Rotate the bulb socket counterclockwise, disconnect the electrical connector and remove.

## Headlamp Bulb Replacement Lo Beam

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the hood in order to access the headlamp bulb accessory covers and headlamp bulbs.

1 | Headlamp Bulb Accessory Cover Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Headlamp Bulb Accessory Cover
3 | Headlamp Bulb Assembly (Low) Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Disconnect the electrical connector and rotate the bulb socket counterclockwise to remove.