For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver or Passenger Seat Replacement.
2. Remove the seat back recliner handle. Refer to Driver or Passenger Seat Recliner Handle Replacement.
3. Remove the seat back recliner cover. Refer to Front Seat Back Recliner Outer Trim Panel Replacement.

1 | Seat Cushion Frame Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Fold the seat back forward to access the bolts. Tighten
25 N·m (18 lb ft)

2 | Seat Outer Adjuster Assembly
3 | Seat Adjuster Handle Assembly Refer to Two-Way Manual Seat Adjuster Handle Replacement.
4 | Seat Adjuster Retaining Spring
5 | Seat Belt Buckle Bolt Tighten 45 N·m (33 lb ft)
6 | Seat Belt Buckle Assembly

#### Procedure

Disconnect the electrical connectors.

7 | Seat Cushion Frame Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
8 | Seat Inner Adjuster Assembly

#### Procedure

Pull up on the adjuster handle and synchronize both the inner and outer adjuster assembly into the same position.