For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement.
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
3. Remove the wiper drive system module. Refer to Windshield Wiper Transmission Replacement.

1 | Windshield Wiper Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4.5 N·m (40 lb in)
2 | Windshield Wiper Motor Assembly Procedure

1. Use the J 39232 Wiper Linkage Separator, or equivalent to separate the transmission arm from the wiper motor crank arm pivot.
2. Use the J 39529 Wiper Linkage Installer, or equivalent to install the transmission arm onto the wiper motor crank arm pivot.

#### Special Tools

• | J 39232 Wiper Linkage Separator

• | J 39529 Wiper Linkage Installer