For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .

1 | Steering Wheel Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 37 N·m (27 lb ft)
2 | Steering Wheel

#### Procedure

1. Disconnect the electrical connectors as needed.
2. Remove the steering wheel using puller J 1859-A with puller legs J 36541-A .
3. Make an alignment mark to note the relationship between the steering wheel and the steering shaft. The marks will be needed to align the wheel during installation.

#### Special Tools

• | J 1859-A Steering Wheel Puller

• | J 36541-A Steering Wheel Puller Legs