For 1990-2009 cars

Product - 88861039, *88861040, High Strength Plastic Repair 50 ml

Components - 12 cartridges with 2 mixers each

Structural and Cosmetic

#### Recommended Repair Material

Product | Components | Recommended Repair Material | Work Time 70°F | Handling Strength at 70°F
--- | --- | --- | --- | ---
88861039 *88861040 High Strength Plastic Repair 50 ml | 12 cartridges with 2 mixers each | Structural and cosmetic bonding and repairing of all flexible plastics. Requires GM P/N 12378462 on TPO plastics. Will also bond e-coated/primed metals. | 90 seconds | 10 minutes
* TPO, TEO, (Polyolefin Plastics) require the application of polyolefin adhesive primer before the GM P/N 88861039 repair compound is applied.

#### Working Time

Product | Adhesive Sandability at 70°F | Part Paintability at 70°F | Adhesive Full Cure at 70°F | Program
--- | --- | --- | --- | ---
88861039 *88861040 High Strength Plastic Repair 50 ml | 20 minutes | 30 minutes | 24 hours | Bumper covers, emblems, door trims, exterior and interior repairs*
* TPO, TEO, (Polyolefin Plastics) require the application of polyolefin adhesive primer before the GM P/N 88861039 repair compound is applied.