For 1990-2009 cars

### Removal Procedure

1. Remove the right floor air outlet duct. Refer to Floor Air Outlet Duct Replacement - Right Side.
2. Remove the blower motor wire harness connector.
3. Remove the blower motor cup bolts (1).
4. Remove the blower motor cup from the blower motor (2).
5. Remove the blower motor bolts (1).
6. Remove the blower motor (2) from the heater case.

### Installation Procedure

1. Install the new blower motor (2) to the heater case.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the blower motor bolts (1) and tighten to XXN·m (XX lb in)..
3. Install the motor blower cup to the blower motor.
4. Install the blower motor cup bolts and tighten to XXN·m (XX lb in)..
5. Install the blower motor wire harness connector.
6. Install the right floor air outlet duct. Refer to Floor Air Outlet Duct Replacement - Right Side.