For 1990-2009 cars

### Removal Procedure

1. Remove instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.
2. Remove instrument panel wiring harness (2) from instrument panel tie bar (1).

Disconnect electrical connectors.

3. Remove instrument panel tie bar (2).

Remove 4 instrument panel tie bar bolts (3, 4).

Remove 2 instrument panel tie bar nuts (1).

4. Remove heater wiring harness.
5. Remove the floor air outlet (2).

Remove the 6 floor air outlet bolts (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the floor air outlet (2).

Install the 6 floor air outlet bolts (1) and tighten to XX N·m (XX lb in).

2. Install heater wiring harness.
3. Install instrument panel tie bar (2).

Install 4 instrument panel tie bar bolts (3, 4) and tighten to XX N·m (XX lb in).

Install 2 instrument panel tie bar nuts (1) and tighten to XX N·m (XX lb in).

4. Attach instrument panel wiring harness (2) to instrument panel tie bar (1).

Connect electrical connectors.

5. Install instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.